HD-XSP-MC3-SystemBuilder-Demo-Program-v2 Release Notes
=========================================================

The HD-XSP-MC3-SystemBuilder-Demo-Program demonstrates the basic functions of the HD-XSP and how they should be programmed in SystemBuilder.
There is no template for the HD-XSP so it has to be custom programmed.
A few signals were omitted from programming to keep the program generic for any device connected to the HD-XSP.
The program consists of an MC3, HD-XSP, TPMC-8X-GA and Xpanel.


The interface has five pages:
Device - consists of information and controls for the device.
Main - consists of information and controls for the Main output.
Downmix - consists of information and controls for the Downmix output.
Decoding - consists of information and controls for the decoding modes.
Source - consists of information and controls for source compensation.



Configuration
===============
This program contains a default IP Table. When loading the system, be sure to load the Default IP Table when prompted by Toolbox.
Also be sure to configure the IP Tables on the devices.
The correct IPIDs are shown below.

IPID 03 - HD-XSP
IPID 04 - TPMC-8X-GA
IPID 05 - Xpanel



Software and Firmware Versions
=============================
Crestron Database ver. 39.00.007.00
Device Database ver. 49.05.004.00
SIMPL Windows ver. 4.02.08.00
SystemBuilder ver. 3.14.006.00
VTPro ver. 5.2.20.00

MC3 ver. 1.007.0016
HD-XSP ver. 1.1969.00001
TPMC-8X-GA ver. 1.00.03.418



Revision History
==================
- v2 - Initial Release