SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    HDBaseT Splitter	3
2.1.1    Basis of Design HDBaseT Splitter:	3
2.1.2    The DA transmitter shall meet the following minimum requirements:	3
3    EXECUTION	4
4    APPENDICES	4
4.1    SPECIFIED PRODUCTS	4
4.1.1    Crestron DM-DA4-4K-C 	4

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	HDBaseT Splitter

2.1.1	Basis of Design HDBaseT Splitter:

2.1.1.1	Crestron DM-DA4-4K-C  

2.1.2	The DA transmitter shall meet the following minimum requirements:

2.1.2.1	Ethernet Port

2.1.2.1.1	One (1) 8-wire RJ-45 

2.1.2.1.1.1	10/100 Mbps, auto-switching, auto negotiating, auto-discovery, full/half duplex, DHCP   

2.1.2.2	One (1) HDMI video, and audio input:

2.1.2.2.1	Supports 4K HDMI 

2.1.2.2.2	Supports DVI-D with adaptor 

2.1.2.2.3	Supports DisplayPort Dual-Mode with adaptor 

2.1.2.2.4	Supports HDCP 2.2 

2.1.2.2.5	Supports Dolby Digital, Dolby Digital EX, Dolby Digital Plus, Dolby TrueHD, Dolby Atmos, DTS, DTS-ES, DTS 96/24, DTS-HD High Res, DTS-HD Master Audio, LPCM up to 8 channels  

2.1.2.3	HDMI digital video/audio output

2.1.2.3.1	One (1) 19-pin Type A HDMI female connector  

2.1.2.4	Four (4) Single UTP/STP cable transmission output:

2.1.2.4.1	Signal transmission up to 330 feet. 

2.1.2.4.2	Supports CAT5e. 

2.1.2.4.3	Supports HDBaseT signal specifications. 

2.1.2.4.4	Supports remote power injection for power HDBaseT receivers.  

2.1.2.5	Power supply modes:

2.1.2.5.1	Local DC power source. 

2.1.2.5.2	Supports sourcing of remote power via an optional power supply.      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS
Specifier Note: This Article includes Crestron products specified in this Guide Specification document. This Article is for reference only and should not be required in actual project manual unless included in an overall system equipment list. 
4.1.1	Crestron DM-DA4-4K-C