adms simpl sample project release notes
=========================================

This program implements an Adagio Digital Media System (ADMS) in use with a PRO2 controller.

The system utilizes the TPMC-8X, TPS-6X, TPMC-3X, APAD and Crestron Mobile user interfaces,
allowing full control of the ADMS Theater and 2 Audio Zones on each interface.



Source Files
=============

Interfaces:
------------
ADMS - TPMC-8x v1.1.2.vtp
ADMS - TPS-6x v1.1.1.vtp
ADMS - TPMC-3x v1.1.1.vtp
ADMS - Crestron Mobile Pro.vtp
ADMS - APAD v1.0.vtp


Programming:
-------------
adms simpl sample project v1.01.03.smw	- SIMPL Windows sample programming
ADMS Speed to String v1.01.usp		- Simpl+ module converts the 3 ADMS zones analog play speeds into a text strings for display.
ADMS Jump Cursor v1.0.usp		- Simpl+ module provides a compact search interface for use with small panels such as the APAD.


Configuration
==============
PRO2 Controller

This program contains a default IP Table. When loading the system, be sure to load the Default IP Table when prompted by Toolbox.
Also be sure to configure the IP tables on the ether net devices to reference the PRO2 controller.
The correct IPIDs are shown below.

Be sure to enabled the controller's web server functionality in order to connect with the Crestron Mobile application.


Ethernet Devices
-----------------
IPID 03 - TPMC-3X
IPID 06 - TPS-6X
IPID 08 - TPMC-8X
IPID 0A - ADMS

Cresnet Devices
----------------
ID 2E - APAD


Settings for Crestron Mobile
-----------------------------
As this program utilizes the Crestron Mobile application for the iPhone or iPod Touch, proper settings must be made to your mobile application.

- Host Name or IP Address:
Set to that of your Pro2 controller.
- HTTP Port:
Set to that of your network (Default 80)
- Port A
Set to that of the programming iPhone and iPod touch Interface Crestron Module (Default 41790)
- Port B
Set to that of the programming iPhone and iPod touch Interface Crestron Module (Default 41791)
Passcode:
1234 (Default)

For further information see Crestron Mobile documentation.


Harbutton functions
--------------------
When available the following hardbutton functions have been included.

Theater & Audio Zone
---------------------
Dpad = OSD Navigation/Browse List Navigation and selection
HOME = Flip to Panel Home page

Transport Controls
►► = Next Track
◄◄ = Previous Track
► = Play
■ = Stop
║= Pause


Theater Only
-------------
MENU = OSD Navigation - Home  = keyboard F12
EXIT = OSD Navigation - Previous Menu = keyboard F11
INFO = Information menu when Video Players active
KEYPAD = Keyboard when Web Browser or Internet TV Active
Side Trigger = Mouse Control when Keyboard Not Enabled


Audio Zones Only
-----------
INFO = Playing information
List = Browse List
Side Trigger = Playing/List toggle


Lights, Climate, Other
--------------------
Transport Control last selected Zone