SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    Wireless Touch Screen User Interface	3
2.1.1    Basis of Design Touch Screen UI:	3
2.1.2    Device Architecture	3
2.1.3    Graphical Display	3
2.1.4    Touch UI Functions	3
2.1.5    Functions - The Touch Screen UI shall include:	3
2.1.6    Communication and Power	4
2.1.7    Physical	4
2.2    Keypad User Interface	4
2.2.1    Basis of Design Control Module:	4
2.2.2    Keypad UI	4
2.2.3    Functions - The Keypad UI shall include:	4
2.2.4    Communication and Power	4
2.2.5    Physical	4
2.3    Speakers - Type 1	4
2.3.1    Basis of Design Speaker:	5
2.3.2    Minimum Requirements:	5
3    EXECUTION	5
4    APPENDICES	5
4.1    SPECIFIED PRODUCTS	5
4.1.1    Crestron TST-902 	6

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	Wireless Touch Screen User Interface

2.1.1	Basis of Design Touch Screen UI:
Specifier Note: Please see system drawings or equipment lists for specified model and quantity.
2.1.1.1	Crestron TST-902 

2.1.1.2	Crestron TST-902-DSW  

2.1.2	Device Architecture

2.1.2.1	The Wireless Touch Screen UI shall be composed of the following functional elements: 

2.1.2.1.1	Graphical touch video display 

2.1.2.1.2	Programmable capacitive buttons   

2.1.3	Graphical Display

2.1.3.1	Graphical UI - Touch screen UI display shall support the following viewable elements:

2.1.3.1.1	Control buttons and objects 

2.1.3.1.2	Feedback indication via text, button object change in color, animated object or graphical element. 

2.1.3.1.3	H.264 or MJPEG Streaming video via WiFi   

2.1.4	Touch UI Functions

2.1.4.1	Touch Screen UI shall support Multi-Touch control interfacing. 

2.1.4.2	Touch Screen UI shall support gesture driven controls through custom programming and configuration.  

2.1.5	Functions - The Touch Screen UI shall include:

2.1.5.1	Custom Control UI - control of integrated system components through custom programming or preset configuration of the system control processor by same manufacturer. 

2.1.5.2	System Integration - device shall support controls for compatible integrated AV systems, HVAC and Lighting hardware, and  scheduling and management systems. 

2.1.5.3	Custom audio feedback via custom programming. 

2.1.5.4	Multi-Language support 

2.1.5.5	Internet Browsing shall be supported via Ethernet network.  
Specifier Note: Internet access required and to be provided by integrator.
2.1.5.6	Voice Recognition - device shall support voice commands control functionality through custom programming and configuratIon of the system control processor.
Specifier Note: Internet access required and to be provided by integrator.
2.1.6	Communication and Power

2.1.6.1	Communication: RF and WiFi 

2.1.6.2	Power:  Included power pack  

2.1.7	Physical

2.1.7.1	Touch Screen UI shall be dockable in an optional wall dock unit.
Specifier Note: Optional wall dock model Crestron TST-902-DSW
2.2	Keypad User Interface

2.2.1	Basis of Design Control Module:
Specifier Note: Please see system drawings or equipment lists for specified model and quantity.
2.2.1.1	Crestron C2N-CBD-P  

2.2.2	Keypad UI

2.2.2.1	Remote Keypad Controls:  Field-configurable remote keypad with auto-adjusting backlight illuminating replaceable, engravable programmable buttons in number indicated, with white LED indicators, configured to fit in standard single-gang box.  

2.2.3	Functions - The Keypad UI shall include:

2.2.3.1	Custom Control UI - control of integrated system components through custom programming or preset configuration of the system control processor by same manufacturer. 

2.2.3.2	System Integration - device shall support controls for compatible integrated AV systems, HVAC and Lighting hardware, and  scheduling and management systems.  

2.2.4	Communication and Power

2.2.4.1	Communication: Wired Network Protocol 

2.2.4.2	Power:  24 VDC integrated with communication cable  

2.2.5	Physical

2.2.5.1	Single gang form factor   

2.3	Speakers - Type 1

2.3.1	Basis of Design Speaker:

2.3.1.1	Crestron SAROS SB-200-P-B  

2.3.2	Minimum Requirements:

2.3.2.1	Stereo amplified sound bar speaker 

2.3.2.2	Performance:

2.3.2.2.1	Output Sensitivity: 83 dB SPL at one meter, both channels driven @ 1-W each 

2.3.2.2.2	Frequency Response: Within plus or minus 3 dB from 100 to 20,000 Hz 

2.3.2.2.3	Go to sleep time: 20 Minutes 

2.3.2.2.4	Amplifier Power: 20 Watts per channel, stereo 

2.3.2.2.5	Woofers: (2) 3 inch polypropylene cone with rubber surround 

2.3.2.2.6	Tweeters: (2) 1 inch polyester dome 

2.3.2.2.7	Passive Radiators: (2) 3 x 4-3/8 inch polypropylene  cone with rubber surround 

2.3.2.2.8	Speaker unit power supply shall be equipped for 100-240 Volts AC, 50/60 Hz power

2.3.2.2.8.1	Maximum power: 50 Watts (500mA)  

2.3.2.2.9	Mounting:

2.3.2.2.9.1	Freestanding: surface or shelf 

2.3.2.2.9.2	Wall mount with included bracket   

2.3.2.3	Enclosures: Plastic housing with perforated metal grill 

2.3.2.4	Connectors:

2.3.2.4.1	Balanced Audio: (1) 5-pin terminal block 

2.3.2.4.2	Unbalanced Audio: (2) RCA female      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron TST-902